Tender text.

Automatic urinal control trap sensor.

Power supply 100 - 240V via AC-adapter or 6V battery.

**Features**:

* Accurate use recognition by detection of urine and water level in the trap
* Automatic flushing after use
* No false flushing by detection of the use instead of the user
* Specially for retrofit situations with back inlet and horizontal drain
* Sensor on the outside of the trap
* Vandal proof flushing system, invisible for the user
* Contactless sensing for maintenance free use recognition
* Water seal monitoring and automatic water seal restoration
* Automatic flushing stop at clogged drain or drain pipes
* 3 flushing programs: eco, normal, full (0,8L; 1,5L; 3L)
* Hygiene flush if not flushed for 24 hours
* Automatic calibration
* E-module IP67

**Delivery**:

* E-module
* Urinal trap with sensor strips
* 6V solenoid valve
* Angle valve with filter and check valve
* Flexible hose with brass back inlet connector and rubber cuff
* Net power adapter or CR-P2 6V battery

**Technical data:**

* EN15091, EN80
* Connect to 100 - 240V, 50 - 60 Hz net power OR CR-P2 6V battery
* Water supply connection: 1/2”
* Drainage connection: ø50mm
* Back inlet & horizontal drain
* Dimensions of the trap with E-module: 120x16x200mm (WxHxD)
* Weight: 1kg